[bookmark: _GoBack]IP Network Audio Encoder                                                                  
FIP-900EC                                                                                                                                          
[image: ]
The IP public address system network audio Encoder is the main equipment of the IP network PA system. It is built-in Encoder which can Encode the analog audio signal into digital and transfer on network.
The IP public address (PA) system key equipment to set up the IP PA sound system, it is convenient to set up sound over network system as one IP Encoder, With this Encoder can easy connect the analog microphone or local DVD or FM into the network.

Feature:
Support to encode analog signal to transfer on IP network .
  Build in SD card player and can transfer the audio over internet.
It is high capacity but cost-effective multiple room network sound system.
The system could be set up over existing network, non dedicated network is needed.
System capacity of more than 500 adapters online simultaneously.
Support LAN/WAN and Internet network.
Network data delay of less than 10 milliseconds.
Program controllable power supply of AC 230V or 110V.


	Model
	IP-900EC

	Description
	IP Network Audio Encoder

	Power Supply
	AC220V or 110V, 50-60Hz

	Power Consumption
	5W

	Network Protocol
	TCP, UDP, ARP, ICMP, IGMP

	Network Speed
	10/100Mbps

	Audio Sampling
	8KHz-48KHz, 16 bits

	Transmission Rate
	8Kbps to 320Kbps

	S/N Ratio
	≥90dB

	Frequency Response
	20Hz-20KHz

	Data Delay
	<20 milliseconds

	Connector
	One RJ45 port for LAN, one aux in, one microphone input, SD port

	Dimensions
	483(W)×256(D)×44(H)mm

	Weight
	2.5kg
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