PA Amplifier with ECHO/USB/SD & FM & Blue Tooth, DC12V                                   
FA-30MD/FA-60MD                                                                                                                                                
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[bookmark: _GoBack]Features:
· Compact mini size public address amplifier
· Ideal for classroom sound system use
· Built-in 100V/70V transformer technology
· Tabletop amplifier with Mp3 player, FM radio & blue tooth
· Rate power output at 30W to 60W . Speaker output of 100V or 70V & 4Ohms-8 Ohms-16 Ohms
· Mp3 player with USB/SD input on front panel, IR remote control for Mp3 player, FM radio and blue tooth
· LED indicators for power, clip, protect and signal
· Mic1-3 and one line. Mic1 of highest priority and one RCA line input and one RCA line output
· Volume control for Mic1-3, line1 and ECHO, Mp3/FM, bass/treble and master
· With short-circuit, clip, overload and high temp protection
· AC220V or 115V & 12V DC both operation system
                                                                                                                                                             
Specification:

	Model
	FA-30MD
FA-120C
FA-240C
	FA-60MD
FA-500C

	Description
	Public Address System 30W Mixer Amplifier

	Rated Power Output
	30W 
120w
240w
	60w
500w

	Speaker Output
	70V, 100V and 4-16Ω

	Input
	Mic1-3: 600 ohms(Ω) 5-8 mV, unbalanced, Line1: 10k ohms(Ω) 150-470 mV,
unbalanced

	Frequency Response
	60-15KHz

	THD
	<0.5% at 1kHz, 1/3 rated power

	S/N Ratio
	Line: 85 dB , MIC: >72 dB

	Protection
	High temp, short circuit, overload protection

	Power Supply
	AC230V or DC12V, 50-60Hz

	Power Consumption
	50W
150W
310W
	80W
650W

	Dimension
	253(W)×220(D)×68(H)mm

	Gross Weight
	4.2kg
6.6kg
9.6kg
	5.3kg
13.7kg

	Warranty
	3 years
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